# Mood.msg — social expression command sent to the LED display node.
#
# mood      : one of "happy", "curious", "annoyed", "playful", "idle"
# intensity : 0.0 (off) to 1.0 (full brightness)

string  mood
float32 intensity
