<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="2.2" y1="0" x2="34.6" y2="0" width="0" layer="20"/>
<wire x1="34.6" y1="0" x2="34.6" y2="47.4" width="0" layer="20"/>
<wire x1="34.6" y1="47.4" x2="2.2" y2="47.4" width="0" layer="20"/>
<wire x1="2.2" y1="47.4" x2="2.2" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="EIA3528-KIT">
<description>&lt;h3&gt;EIA3528-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
<package name="0805">
</package>
<package name="LUXEON-PAD">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
</packages>
</library>
<library name="DWM1000">
<packages>
<package name="DWM1000">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun" package="SOT223" value=""/>
<element name="C1" library="SparkFun" package="EIA3528-KIT" value=""/>
<element name="C2" library="SparkFun" package="EIA3528-KIT" value=""/>
<element name="R1" library="SparkFun" package="0805" value=""/>
<element name="JP1" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="U2" library="SparkFun" package="TQFP32-08" value="ATMEGA168"/>
<element name="JP2" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP3" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP4" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP5" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="R2" library="SparkFun" package="0805" value=""/>
<element name="JP7" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP8" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP9" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP6" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP10" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP11" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP12" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP13" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP14" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="JP15" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="X1" library="SparkFun" package="USB-MICROB" value="USB-MICROB"/>
<element name="JP16" library="SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="U$1" library="DWM1000" package="DWM1000" value="DWM1000"/>
</elements>
<signals>
<signal name="VCC3.3">
<contactref element="C1" pad="A"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP15" pad="P$1"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="20"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="VDDAON"/>
<contactref element="U$1" pad="VDD3V3"/>
<contactref element="U$1" pad="VDD3V3.2"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="C"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="C"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="21"/>
<contactref element="R2" pad="1"/>
<contactref element="X1" pad="GND"/>
<contactref element="JP16" pad="P$1"/>
<contactref element="U$1" pad="VSS"/>
<contactref element="U$1" pad="VSS.2"/>
<contactref element="U$1" pad="VSS.3"/>
<contactref element="U$1" pad="VSS.4"/>
<contactref element="U$1" pad="VSS.5"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="A"/>
<contactref element="JP14" pad="P$1"/>
<contactref element="X1" pad="VBUS"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="7"/>
<contactref element="JP1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="8"/>
<contactref element="JP2" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="31"/>
<contactref element="JP4" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="30"/>
<contactref element="JP5" pad="P$1"/>
</signal>
<signal name="IRQ">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="32"/>
<contactref element="U$1" pad="IRQ/GPIO8"/>
</signal>
<signal name="CLK">
<contactref element="U2" pad="17"/>
<contactref element="JP10" pad="P$1"/>
<contactref element="JP6" pad="P$1"/>
<contactref element="U$1" pad="SPICLK"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="16"/>
<contactref element="JP7" pad="P$1"/>
<contactref element="JP11" pad="P$1"/>
<contactref element="U$1" pad="SPIMISO"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="15"/>
<contactref element="JP8" pad="P$1"/>
<contactref element="JP12" pad="P$1"/>
<contactref element="U$1" pad="SPIMOSI"/>
</signal>
<signal name="CSN">
<contactref element="U2" pad="14"/>
<contactref element="JP9" pad="P$1"/>
<contactref element="JP13" pad="P$1"/>
<contactref element="U$1" pad="SPICSN"/>
</signal>
<signal name="RESET">
<contactref element="U2" pad="13"/>
<contactref element="U$1" pad="RST"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
</signals>
</board>
</drawing>
</eagle>
