<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<library>
<packages>
<package name="DWM1000">
</package>
</packages>
<symbols>
<symbol name="DWM1000">
<pin name="EXTON" direction="out"/>
<pin name="WAKEUP"/>
<pin name="!RST" direction="in"/>
<pin name="GPIO7"/>
<pin name="VDDAON"/>
<pin name="VDD" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="VDD@2" direction="pas"/>
<pin name="VSS@2" direction="pas"/>
<pin name="VSS@3" direction="pas"/>
<pin name="IRQ/GPIO8"/>
<pin name="VSS@4" direction="pas"/>
<pin name="SPICLK" direction="in"/>
<pin name="SPIMISO" direction="out"/>
<pin name="SPIMOSI" direction="in"/>
<pin name="!SPICS" direction="in"/>
<pin name="GPIO6"/>
<pin name="GPIO5/SPIPOL"/>
<pin name="GPIO4"/>
<pin name="GPIO3/TXLED"/>
<pin name="GPIO2/RXLED"/>
<pin name="GPIO1/SFDLED"/>
<pin name="GPIO0/RXOKLED"/>
<pin name="VSS@5"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DWM1000" prefix="U">
<description>The DWM1000 module is based on Decawave's DW1000 Ultra
Wideband (UWB) transceiver IC. It integrates antenna, all RF
circuitry, power management and clock circuitry in one module.
It can be used in 2-way ranging or TDOA location systems to
locate assets to a precision of 10 cm and supports data rates of
up to 6.8 Mbps</description>
<gates>
<gate name="G$1" symbol="DWM1000"/>
</gates>
<devices>
<device name="" package="DWM1000">
<connects>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!SPICS" pad="17"/>
<connect gate="G$1" pin="EXTON" pad="1"/>
<connect gate="G$1" pin="GPIO0/RXOKLED" pad="15"/>
<connect gate="G$1" pin="GPIO1/SFDLED" pad="14"/>
<connect gate="G$1" pin="GPIO2/RXLED" pad="13"/>
<connect gate="G$1" pin="GPIO3/TXLED" pad="12"/>
<connect gate="G$1" pin="GPIO4" pad="11"/>
<connect gate="G$1" pin="GPIO5/SPIPOL" pad="10"/>
<connect gate="G$1" pin="GPIO6" pad="9"/>
<connect gate="G$1" pin="GPIO7" pad="4"/>
<connect gate="G$1" pin="IRQ/GPIO8" pad="22"/>
<connect gate="G$1" pin="SPICLK" pad="20"/>
<connect gate="G$1" pin="SPIMISO" pad="19"/>
<connect gate="G$1" pin="SPIMOSI" pad="18"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="6"/>
<connect gate="G$1" pin="VDDAON" pad="5"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="24"/>
<connect gate="G$1" pin="VSS@3" pad="23"/>
<connect gate="G$1" pin="VSS@4" pad="21"/>
<connect gate="G$1" pin="VSS@5" pad="16"/>
<connect gate="G$1" pin="WAKEUP" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
